TOWN OF HANCOCK

P.O. BOX 100

HANCOCK, VERMONT 05748

TELEPHONE (802)767-3660

# Prospectus For Tucker Brook Road

## Ditch Cleaning/Shaping and Stone Lining

## 6/21/2024

**The Town of Hancock, Vermont is seeking construction bids for ditch cleaning, shaping and lining on Tucker Brook Road in Hancock, Vermont.**

**Insurance Requirements:** The Town of Hancock requires that all Contractors or Persons working for the Town of Hancock carry a General liability Policy of no less than One million Dollars ($1,000,000.00) **with the Town of Hancock being an additional Insured.** Any Contractor or Persons working for the Town of Hancock having Employees must provide the Town of Hancock with a Certificate of Worker’s Compensation meeting all State of Vermont and Federal Statues. **All Insurance Certificates must be on file with the Hancock Town Clerk** **before work is to begin.**

**Additional Requirements:** The Town of Hancock requires that any Vehicle exceeding the twenty four thousand pound weight limit (24,000) with or without load, obtain an overweight permit. The Town of Hancock has restrictions on its roads and obtaining this permit is the only way to operate legally on the Hancock Road System.

**Additional Requirement:** The Town of Hancock requires that all construction sites be properly warned with the correct signage and cones.

**Additional Requirement:** The Town of Hancock requires that the Contractor provide Traffic control as needed.

**Additional Requirement:** Contractor shall call Dig Safe prior to starting any work.

**Contractor Responsibilities:** Furnish all Equipment, Materials, Insurances, Labor and Knowledge necessary to complete the project described herein within the timeframe allowed.

**Town of Hancock’s Responsibilities:** Direction so the herein described project can be completed in the timeframe allowed.

**Location:** There are two separate sections of ditch receiving work through this contract.

The first worksite is located approximately .4 miles north on Tucker Brook Rd. from the intersection of Tucker Brook Rd. and Route 125. The area to receive ditch work is on the right (east) side of Tucker Brook Rd. The worksite starts at the intersection of Tucker Brook Rd. and Tucker Brook Extension and extends along Tucker Brook Rd. for a distance of 470 linear feet. This section of ditch is marked at each end with stakes with orange marking tape. This worksite starts at 43.930710, -72.864302 and ends at 43.931659, -72.865572.

The second worksite is located approximately 1.0 miles up Tucker Brook Road from the intersection with VT Route 125. Ditch repairs begin at the intersection of Tucker Brook Rd. and Windigo Rd. This section extends 510 feet up (north) Tucker Brook Road along the right (east) side of the road. The worksite is marked at each end with stakes with orange marking tape. This worksite starts at 43.938339, -72.865073 and ends at 43.939381, -72.866247.

## Materials:

1. 7” Erosion Stone (Quantities to be determined by contractor based on drawing provided by the Town of Hancock)
2. 1 ½” Clean Stone NO FINES (Quantities to be determined by Contractor based on drawings provided by the Town of Hancock.
3. Filter fabric for entire length of project.
4. The Town of Hancock requires that all bare ground including any areas provided for the waste materials from the ditch cleaning be hydroseeded or seeded and mulched with a Contractor’s Mix. All bare ground must be covered post construction.

## Description of Work:

**Ditch Work:**

1. Contractor shall clean and shape the ditch area. At a minimum, the Town of Hancock requires the base width to be 2’. The depth of the ditch should be 4’ at the center line with the base of Tucker Brook Rd. as a completion height. Exceptions to these requirements will be considered by the Road Commissioner in the event that ledge is encountered. All stone must be 6” below the edge of Tucker Brook Rd. **See Diagram on last page.**
2. **It shall be the Contractor’s responsibility to remove all excess materials generated from this project.**
3. Once the ditch has been cleaned and shaped the Contractor shall place the filter fabric followed by the 1½” clean stone in the ditch, keeping the clean stone 6” below the side of the road. The bank side shall have the same clean stone height requirement.
4. Place 7” ditch stone to a minimum depth of 4’ across the base width, then stone the side slopes of the ditch to the required height.
5. Reset any existing bank retaining stones as needed. Any exposed bank soils not covered with retaining stones shall be covered as stated above.
6. Culvert entrances and exits shall be cleaned, shaped, and lined as needed.

### Resolution of Disputes:

The Town of Hancock and the winning Contractor agree to hire an independent arbitrator to settle any and all disputes that may arise. Both parties will share the expense of an arbitrator equally.

### Warranty of work performed:

Contractor will guarantee work performed to the full satisfaction of the Hancock Road Commissioner and the Hancock Select Board for a period of not less than one full year (12 months) from the date of the final inspection. This guarantee shall cover all workmanship and any materials the Contractor supplied. In the event of a failure in any of the workmanship or materials, the Contractor will, at their expense, replace or redo any part that has failed and any other damages that may have occurred because of that failure.

This project will be overseen by the Hancock Road Commissioner all inquiries are to be directed to the Road Commissioner (Derek Dzhugashvili 631.487.1823). If the Road Commissioner is unavailable, you may direct your question to the Hancock Select Board Chair (Scott Gillette 802.770.0727).

### Project completion date:

October 31th, 2024

### Bid Format:

Bid shall be submitted in writing on the attached bid sheet as a single lump sum amount for the project. Bids not conforming to this format shall be rejected.

### Bids due:

**Tuesday, July 16, 2024 by 3:00 PM at the Hancock Town Clerk’s office.**

Bids may be hand delivered to the Hancock Town Clerk’s office for drop off in the outside drop box or Bids may be mailed, so long as they are **received** any time before 3pm on Tuesday July 16, 2024. All Bids shall be in a sealed envelope marked, **Tucker Brook Rd Ditching / Town of Hancock.**

Bids submitted via postal service shall be addressed to **Town of Hancock, Tucker Brook Rd Ditching, PO Box 100, Hancock, VT 05748.**

**Bids submitted via email or other electronic means shall be rejected.**

### THE TOWN OF HANCOCK RESERVES THE RIGHT TO REJECT ANY AND ALL BIDS.

# By order of the Hancock Selectboard

## Bid and Signature Sheet for Hancock Road Projects

\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ submits the following bid based on the prospectus provided by the Town of Hancock. It is further understood that by submitting this bid I/we agree to all the terms described herein. It is furthermore understood that construction projects have many variables and extras and changes may be made as the project proceeds. We agree to work with the Town of Hancock on all changes. We further agree that all changes will be agreed to in writing before any work is to proceed.

BID AMOUNT SUBMITTED:\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

DATE:\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

For 2024 Tucker Brook Rd Ditch Cleaning / Shaping Project.

Signatures of company’s authorized agents:

\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Bidder’s phone and Email contact information

\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

## The Town of Hancock hereby accepts the bid submitted by:

\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ ON \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

The Hancock selectboard agrees to the terms stated within this prospectus and further agrees that the above named company may begin work as stated within.

## Hancock Selectboard:

\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ DATED:\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

